**Ansible problem statements.(VLAN)**

1. **Create VLAN configuration on below 3 switches. And print the result of ‘show vlan’ before and after creation vlan. (hint:- create input into inventory as host vars for below variables )**

**configuration for S1**

vlan\_id: 400

vlan\_name: vlan\_2400

interfaces: ‘[“Gi0/1”,” Gi0/2”.” Gi1/3”]’

delay: 15

state: present

**configuration for S2**

vlan\_id: 500

vlan\_name: vlan\_test\_500

interfaces: ‘[“Gi0/1”]’

state: present

**configuration for S3**

vlan\_id: 400

vlan\_name: vlan\_test\_400

state: present

1. **Write a another playbook to delete the above created VLANs(use state absent)**